IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2017-01-17T15:44:39"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20150220_1215(x64) - Exporter 16.0.428.0 - Default UI"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "1201238" of Organization (no name given)
  Owner history of Person "1201238" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 1482415221 (2016-12-22T14:00:21Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Surface:1111047" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "1.krs Lattia" | long name "1.krs Lattia" | elevation 4750.
        contains 365 elements
          85 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:AR1311_VS NKH 130mm" | object type "Basic Wall:AR1311_VS NKH 130mm:227484" | names: "Basic Wall:AR1311_VS NKH 130mm:437285", "Basic Wall:AR1311_VS NKH 130mm:537749", "Basic Wall:AR1311_VS NKH 130mm:559340" (+82 more) | material: layers "Basic Wall:AR1311_VS NKH 130mm" ("Brick, WHITE" 130.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:531880" | material: "Brick, WHITE" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:537490" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:537526" | material: "Brick, WHITE" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:537551" | material: "Brick, WHITE" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:537631" | material: "Brick, GRAY" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          24 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:AR1312_VS-LASI" | object type "Curtain Wall:AR1312_VS-LASI:382" | names: "Curtain Wall:AR1312_VS-LASI:552523", "Curtain Wall:AR1312_VS-LASI:558170", "Curtain Wall:AR1312_VS-LASI:558721" (+21 more) | parts: 219 IFCMEMBER, 64 IFCPLATE | property sets: Pset_CurtainWallCommon, Constraints, Dimensions, Horizontal Grid, Other, Phasing
          2 x IFCDOOR | type IFCDOORSTYLE "9 x 20 M" | object type "9 x 20 M" | names: "1315_VÄLIOVI Iso lasiaukko:9 x 20 M:560063", "1315_VÄLIOVI Iso lasiaukko:9 x 20 M:560887" | material: materials ("Cherry", "Metal - Stainless Steel", "Metal - Painted - Grey", "Glass") | property sets: Pset_DoorCommon, Constraints, Construction, Dimensions, Identity Data, Other
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:AR1241_US 1 420mm" | object type "Basic Wall:AR1241_US 1 420mm:1739" | names: "Basic Wall:AR1241_US 1 420mm:902582", "Basic Wall:AR1241_US 1 420mm:902810", "Basic Wall:AR1241_US 1 420mm:903567" (+7 more) | material: layers "Basic Wall:AR1241_US 1 420mm" ("Brick, GRAY" 90., "Air" 40., "Plywood, Sheathing" 30., "Concrete - Cast-in-Place Concrete" 170., "Brick, WHITE" 90.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:903772" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:904164" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:904354" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:904459" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:904576" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:904751" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:904848" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:904971" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:905108" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:905203" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:905278" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:905365" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:905448" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:905561" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:905656" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:906298" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:906598" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:906645" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:906740" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:906877" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:906938" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:906993" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:907052" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:907119" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:907172" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:907235" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:907288" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:907361" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:907406" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:907463" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:907504" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:907641" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:907718" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:907795" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:907888" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:907953" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:908018" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:908083" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:908140" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:908201" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:908252" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:908313" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:908380" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:908435" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:908518" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:908597" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:908680" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:AR1311_VS NKH 130mm" | object type "Basic Wall:AR1311_VS NKH 130mm:227484" | names: "Basic Wall:AR1311_VS NKH 130mm:912783", "Basic Wall:AR1311_VS NKH 130mm:927903" | material: layers "Basic Wall:AR1311_VS NKH 130mm" ("Brick, WHITE" 130.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:AR1212_PERUSMUURI" | object type "Basic Wall:AR1212_PERUSMUURI:1755" | names: "Basic Wall:AR1212_PERUSMUURI:914421", "Basic Wall:AR1212_PERUSMUURI:914784", "Basic Wall:AR1212_PERUSMUURI:914927" (+7 more) | material: layers "Basic Wall:AR1212_PERUSMUURI" ("Concrete, Cast In Situ" 150., "Mineral Wool" 76., "Concrete, Cast In Situ" 150.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:AR1311_VS Betoni 160mm" | object type "Basic Wall:AR1311_VS Betoni 160mm:513742" | names: "Basic Wall:AR1311_VS Betoni 160mm:917818", "Basic Wall:AR1311_VS Betoni 160mm:918011", "Basic Wall:AR1311_VS Betoni 160mm:918270" (+3 more) | material: layers "Basic Wall:AR1311_VS Betoni 160mm" ("Concrete, Cast In Situ" 160.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          14 x IFCDOOR | type IFCDOORSTYLE "9 x 21 M" | object type "9 x 21 M" | names: "1315_VÄLIOVI Puu, umpi:9 x 21 M:920526", "1315_VÄLIOVI Puu, umpi:9 x 21 M:920822", "1315_VÄLIOVI Puu, umpi:9 x 21 M:920878" (+11 more) | material: materials ("Door - Frame White", "Door - Panel White") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          15 x IFCDOOR | type IFCDOORSTYLE "9 x 21 M" | object type "9 x 21 M" | names: "1315_VÄLIOVI Puu, umpi:9 x 21 M:920580", "1315_VÄLIOVI Puu, umpi:9 x 21 M:921056", "1315_VÄLIOVI Puu, umpi:9 x 21 M:921162" (+12 more) | material: materials ("Door - Frame White", "Door - Panel White") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "9 x 21 M" | object type "9 x 21 M" | names: "1315_VÄLIOVI Puu, umpi:9 x 21 M:920780" | material: materials ("Door - Panel White", "Door - Frame White") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCDOOR | type IFCDOORSTYLE "7 x 21 M" | object type "7 x 21 M" | names: "1315_VÄLIOVI Puu, umpi:7 x 21 M:922781", "1315_VÄLIOVI Puu, umpi:7 x 21 M:922819", "1315_VÄLIOVI Puu, umpi:7 x 21 M:923278" | material: materials ("Door - Frame White", "Door - Panel White") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCDOOR | type IFCDOORSTYLE "9 x 21 M" | object type "9 x 21 M" | names: "1315_VÄLIOVI Puu, umpi:9 x 21 M:923096", "1315_VÄLIOVI Puu, umpi:9 x 21 M:923141" | material: materials ("Door - Frame White", "Door - Panel White") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          5 x IFCDOOR | type IFCDOORSTYLE "8 x 21 M" | object type "8 x 21 M" | names: "1315_VÄLIOVI Puu, umpi:8 x 21 M:923394", "1315_VÄLIOVI Puu, umpi:8 x 21 M:923562", "1315_VÄLIOVI Puu, umpi:8 x 21 M:934226" (+2 more) | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:924538", "AR1233_PILARI Pyöreä,betoni:300mm:924771", "AR1233_PILARI Pyöreä,betoni:300mm:924868" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:925875" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:926112" | material: "Brick, WHITE" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:926219" | material: "Brick, WHITE" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:926431" | material: "Brick, WHITE" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:926469" | material: "Brick, WHITE" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:926491" | material: "Brick, GRAY" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:926508" | material: "Brick, GRAY" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:927290" | material: "Brick, GRAY" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300mm" | object type "300mm" | names: "AR1233_PILARI Pyöreä,betoni:300mm:927346" | material: "Brick, GRAY" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:929290" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Materials and Finishes, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:929541" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Materials and Finishes, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:929628" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Materials and Finishes, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:929652" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Materials and Finishes, Other, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "380 x 380mm" | object type "380 x 380mm" | names: "AR1233_PILARI Betoni, neliö:380 x 380mm:929690" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Constraints, Dimensions, Materials and Finishes, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:AR1311_VS Betoni 210mm" | object type "Basic Wall:AR1311_VS Betoni 210mm:281739" | names: "Basic Wall:AR1311_VS Betoni 210mm:930398" | material: layers "Basic Wall:AR1311_VS Betoni 210mm" ("Concrete, Cast In Situ" 210.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:AR1311_VS Betoni 300mm" | object type "Basic Wall:AR1311_VS Betoni 300mm:423507" | names: "Basic Wall:AR1311_VS Betoni 300mm:930678" | material: layers "Basic Wall:AR1311_VS Betoni 300mm" ("Concrete, Cast In Situ" 300.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:AR1311_VS Betoni 420mm" | object type "Basic Wall:AR1311_VS Betoni 420mm:233516" | names: "Basic Wall:AR1311_VS Betoni 420mm:930915", "Basic Wall:AR1311_VS Betoni 420mm:931892", "Basic Wall:AR1311_VS Betoni 420mm:961099" (+3 more) | material: layers "Basic Wall:AR1311_VS Betoni 420mm" ("Concrete, Cast In Situ" 420.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:AR1311_VS Betoni 200mm" | object type "Basic Wall:AR1311_VS Betoni 200mm:657428" | names: "Basic Wall:AR1311_VS Betoni 200mm:933201" | material: layers "Basic Wall:AR1311_VS Betoni 200mm" ("Concrete, Cast In Situ" 200.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "9 x 21 M" | object type "9 x 21 M" | names: "1315_VÄLIOVI Puu, umpi:9 x 21 M:933242" | material: materials ("Door - Frame White", "Door - Panel White") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:AR1311_VS Metalli, levyverhous 105mm" | object type "Basic Wall:AR1311_VS Metalli, levyverhous 105mm:570172" | names: "Basic Wall:AR1311_VS Metalli, levyverhous 105mm:933387", "Basic Wall:AR1311_VS Metalli, levyverhous 105mm:963855", "Basic Wall:AR1311_VS Metalli, levyverhous 105mm:1009470" (+2 more) | material: layers "Basic Wall:AR1311_VS Metalli, levyverhous 105mm" ("Stainless Steel" 2.5, "Steel, 45-345" 100., "Stainless Steel" 2.5) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "8 x 21 M" | object type "8 x 21 M" | names: "1315_VÄLIOVI Puu, umpi:8 x 21 M:933462" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "8 x 21 M" | object type "8 x 21 M" | names: "1315_VÄLIOVI Puu, umpi:8 x 21 M:934362" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "9 x 21 M" | object type "9 x 21 M" | names: "1315_VÄLIOVI Puu, umpi:9 x 21 M:934944" | material: materials ("Door - Frame White", "Door - Panel White") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "10 x 22 M" | object type "10 x 22 M" | names: "1315_VÄLIOVI Puu, umpi:10 x 22 M:935023" | material: materials ("Door - Frame White", "Door - Panel White") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          6 x IFCSLAB | object type "Floor:AR1235_VP Betoni 120mm" | FLOOR | names: "Floor:AR1235_VP Betoni 120mm:936724", "Floor:AR1235_VP Betoni 120mm:1124210", "Floor:AR1235_VP Betoni 120mm:1124239" (+3 more) | material: layers "Floor:AR1235_VP Betoni 120mm" ("Default Floor" 120.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "15 x 22 M" | object type "15 x 22 M" | names: "1315_VÄLIOVI Umpipariovi:15 x 22 M:939756" | material: materials ("Puu - tammi, höylätty", "NCS S 1502-G50Y Helmenharmaa, matta, ruisku") | property sets: Pset_DoorCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Graphics, Identity Data
          9 x IFCBEAM | object type "AR1234_PALKKI Betoni, suorakaide:380 x 520mm 2:1051496" | names: "AR1234_PALKKI Betoni, suorakaide:380 x 520mm 2:946421", "AR1234_PALKKI Betoni, suorakaide:380 x 520mm 2:946498", "AR1234_PALKKI Betoni, suorakaide:380 x 520mm 2:946543" (+6 more) | material: "Concrete, Cast-in-Place gray"; materials ("Concrete, Cast In Situ", "Concrete, Cast-in-Place gray") | property sets: Pset_BeamCommon, Constraints, Dimensions, Geometric Position, Materials and Finishes, Other
          2 x IFCSTAIR | object type "Precast Stair:AR1237_PORRAS Betoni:107948" | names: "Precast Stair:Stair:953595", "Precast Stair:Stair:981745" | parts: 4 IFCRAILING, 2 IFCSTAIRFLIGHT | property sets: Pset_StairCommon, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:AR1313_VS-ERITYIS Kevyt väliseinä, metalli runko" | object type "Curtain Wall:AR1313_VS-ERITYIS Kevyt väliseinä, metalli runko:548469" | names: "Curtain Wall:AR1313_VS-ERITYIS Kevyt väliseinä, metalli runko:963456", "Curtain Wall:AR1313_VS-ERITYIS Kevyt väliseinä, metalli runko:963736" | parts: 44 IFCMEMBER, 16 IFCPLATE | property sets: Pset_CurtainWallCommon, Constraints, Dimensions, Horizontal Grid, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "18 x 21 M" | object type "18 x 21 M" | names: "1315_VÄLIOVI Pariovi kaksi lasiaukkoa:18 x 21 M:963938" | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Pset_DoorCommon, Constraints, Construction, Dimensions, Identity Data, Other
          5 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:AR1245_LASIUS" | object type "Curtain Wall:AR1245_LASIUS:614557" | names: "Curtain Wall:AR1245_LASIUS:986164", "Curtain Wall:AR1245_LASIUS:986867", "Curtain Wall:AR1245_LASIUS:987184" (+2 more) | parts: 35 IFCMEMBER, 10 IFCPLATE | property sets: Pset_CurtainWallCommon, Constraints, Dimensions, Horizontal Grid, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "19 x 21 M" | object type "19 x 21 M" | names: "1315_VÄLIOVI Pariovi kaksi lasiaukkoa:19 x 21 M:1009814" | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Pset_DoorCommon, Constraints, Construction, Dimensions, Identity Data, Other
          1 x IFCDOOR | type IFCDOORSTYLE "16 x 22 M" | object type "16 x 22 M" | names: "1315_VÄLIOVI Pariovi kaksi lasiaukkoa:16 x 22 M:1010881" | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Pset_DoorCommon, Constraints, Construction, Dimensions, Identity Data, Other
          1 x IFCDOOR | type IFCDOORSTYLE "18 x 21 M" | object type "18 x 21 M" | names: "1315_VÄLIOVI Pariovi kaksi lasiaukkoa:18 x 21 M:1028795" | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Pset_DoorCommon, Constraints, Construction, Dimensions, Identity Data, Other
          1 x IFCDOOR | type IFCDOORSTYLE "19 x 21 M" | object type "19 x 21 M" | names: "1315_VÄLIOVI Pariovi kaksi lasiaukkoa:19 x 21 M:1029766" | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Pset_DoorCommon, Constraints, Construction, Dimensions, Identity Data, Other
          28 x IFCWINDOW | type IFCWINDOWSTYLE "21 x 17 M 2" | object type "21 x 17 M 2" | names: "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1030634", "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1030868", "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1031008" (+25 more) | material: "Glass" | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCWINDOW | type IFCWINDOWSTYLE "21 x 15 M 2" | object type "21 x 15 M 2" | names: "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 15 M 2:1050272", "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 15 M 2:1050876", "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 15 M 2:1050960" | material: "Glass" | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          29 x IFCWINDOW | type IFCWINDOWSTYLE "21 x 17 M 2" | object type "21 x 17 M 2" | names: "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1063054", "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1063093", "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1065660" (+26 more) | material: "Glass" | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "6 x 6 M" | object type "6 x 6 M" | names: "AR1242_IKKUNA:6 x 6 M:1073260" | material: materials ("Glass", "Sash") | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "6 x 6 M" | object type "6 x 6 M" | names: "AR1242_IKKUNA:6 x 6 M:1073400" | material: materials ("Glass", "Sash") | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "10 x 23 M" | object type "10 x 23 M" | names: "1243_ULKOOVI Iso lasiaukolla:10 x 23 M:1082471" | material: materials ("Cherry", "Metal - Stainless Steel", "Finish - White", "Glass") | property sets: Pset_DoorCommon, Constraints, Construction, Dimensions, Identity Data, Other
          1 x IFCWINDOW | type IFCWINDOWSTYLE "5 x 15 M 2" | object type "5 x 15 M 2" | names: "AR1242_IKKUNA:5 x 15 M 2:1086714" | material: materials ("Glass", "Sash") | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:AR1311_VS Puu 140mm" | object type "Basic Wall:AR1311_VS Puu 140mm:1753" | names: "Basic Wall:AR1311_VS Puu 140mm:1120608", "Basic Wall:AR1311_VS Puu 140mm:1120766" | material: layers "Basic Wall:AR1311_VS Puu 140mm" ("Gypsum Wall Board" 21., "Softwood, Lumber" 98., "Gypsum Wall Board" 21.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCSLAB | object type "Floor:AR1236_YP Betoni 200mm, eriste 150m" | FLOOR | names: "Floor:AR1236_YP Betoni 200mm, eriste 150m:1132319" | material: layers "Floor:AR1236_YP Betoni 200mm, eriste 150m" ("Mineral Wool" 150., "Default Floor" 200.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCROOF | object type "Basic Roof:AR1261_VK-RAKENNE Huopakatto, rakenne 125mm:1400" | names: "Basic Roof:AR1261_VK-RAKENNE Huopakatto, rakenne 125mm:1134136" | material: "Metal Stud Layer" | property sets: Pset_RoofCommon, Constraints, Construction, Dimensions, Other, Phasing
      IFCBUILDINGSTOREY "2.krs Lattia" | long name "2.krs Lattia" | elevation 8150.
        contains 214 elements
          4 x IFCSLAB | object type "Floor:AR1235_VP Betoni 120mm" | FLOOR | names: "Floor:AR1235_VP Betoni 120mm:938250", "Floor:AR1235_VP Betoni 120mm:994375", "Floor:AR1235_VP Betoni 120mm:1115714" (+1 more) | material: layers "Floor:AR1235_VP Betoni 120mm" ("Default Floor" 120.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Other, Phasing, Structural
          54 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:AR1311_VS NKH 130mm" | object type "Basic Wall:AR1311_VS NKH 130mm:227484" | names: "Basic Wall:AR1311_VS NKH 130mm:939961", "Basic Wall:AR1311_VS NKH 130mm:940360", "Basic Wall:AR1311_VS NKH 130mm:940464" (+51 more) | material: layers "Basic Wall:AR1311_VS NKH 130mm" ("Brick, WHITE" 130.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          14 x IFCDOOR | type IFCDOORSTYLE "9 x 21 M" | object type "9 x 21 M" | names: "1315_VÄLIOVI Puu, umpi:9 x 21 M:943263", "1315_VÄLIOVI Puu, umpi:9 x 21 M:944159", "1315_VÄLIOVI Puu, umpi:9 x 21 M:944207" (+11 more) | material: materials ("Door - Frame White", "Door - Panel White") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          16 x IFCDOOR | type IFCDOORSTYLE "9 x 21 M" | object type "9 x 21 M" | names: "1315_VÄLIOVI Puu, umpi:9 x 21 M:943309", "1315_VÄLIOVI Puu, umpi:9 x 21 M:943343", "1315_VÄLIOVI Puu, umpi:9 x 21 M:943399" (+13 more) | material: materials ("Door - Frame White", "Door - Panel White") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "15 x 22 M" | object type "15 x 22 M" | names: "1315_VÄLIOVI Umpipariovi:15 x 22 M:952544" | material: materials ("Puu - tammi, höylätty", "NCS S 1502-G50Y Helmenharmaa, matta, ruisku") | property sets: Pset_DoorCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Graphics, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "6 x 21 M" | object type "6 x 21 M" | names: "1315_VÄLIOVI Puu, umpi:6 x 21 M:952607" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "19 x 21 M" | object type "19 x 21 M" | names: "1315_VÄLIOVI Pariovi kaksi lasiaukkoa:19 x 21 M:954973" | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Pset_DoorCommon, Constraints, Construction, Dimensions, Identity Data, Other
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:AR1311_VS Metalli, levyverhous 105mm" | object type "Basic Wall:AR1311_VS Metalli, levyverhous 105mm:570172" | names: "Basic Wall:AR1311_VS Metalli, levyverhous 105mm:955088", "Basic Wall:AR1311_VS Metalli, levyverhous 105mm:972427", "Basic Wall:AR1311_VS Metalli, levyverhous 105mm:972957" | material: layers "Basic Wall:AR1311_VS Metalli, levyverhous 105mm" ("Stainless Steel" 2.5, "Steel, 45-345" 100., "Stainless Steel" 2.5) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "16 x 22 M" | object type "16 x 22 M" | names: "1315_VÄLIOVI Pariovi kaksi lasiaukkoa:16 x 22 M:955166" | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Pset_DoorCommon, Constraints, Construction, Dimensions, Identity Data, Other
          2 x IFCDOOR | type IFCDOORSTYLE "16 x 22 M" | object type "16 x 22 M" | names: "1315_VÄLIOVI Pariovi kaksi lasiaukkoa:16 x 22 M:972686", "1315_VÄLIOVI Pariovi kaksi lasiaukkoa:16 x 22 M:973046" | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Pset_DoorCommon, Constraints, Construction, Dimensions, Identity Data, Other
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:AR1241_US 1 420mm" | object type "Basic Wall:AR1241_US 1 420mm:1739" | names: "Basic Wall:AR1241_US 1 420mm:978564", "Basic Wall:AR1241_US 1 420mm:978666", "Basic Wall:AR1241_US 1 420mm:978811" (+4 more) | material: layers "Basic Wall:AR1241_US 1 420mm" ("Brick, GRAY" 90., "Air" 40., "Plywood, Sheathing" 30., "Concrete - Cast-in-Place Concrete" 170., "Brick, WHITE" 90.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "8 x 22 M" | object type "8 x 22 M" | names: "1315_VÄLIOVI Puu, umpi:8 x 22 M:980131" | material: materials ("Door - Frame White", "Door - Panel White") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:AR1311_VS Betoni 160mm" | object type "Basic Wall:AR1311_VS Betoni 160mm:513742" | names: "Basic Wall:AR1311_VS Betoni 160mm:996494" | material: layers "Basic Wall:AR1311_VS Betoni 160mm" ("Concrete, Cast In Situ" 160.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          8 x IFCBEAM | object type "AR1234_PALKKI Betoni, suorakaide:380 x 520mm 2:1051496" | names: "AR1234_PALKKI Betoni, suorakaide:380 x 520mm 2:1001215", "AR1234_PALKKI Betoni, suorakaide:380 x 520mm 2:1001305", "AR1234_PALKKI Betoni, suorakaide:380 x 520mm 2:1001428" (+5 more) | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Constraints, Dimensions, Geometric Position, Identity Data, Materials and Finishes
          20 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:AR1312_VS-LASI" | object type "Curtain Wall:AR1312_VS-LASI:382" | names: "Curtain Wall:AR1312_VS-LASI:1009157", "Curtain Wall:AR1312_VS-LASI:1014621", "Curtain Wall:AR1312_VS-LASI:1014715" (+17 more) | parts: 140 IFCMEMBER, 40 IFCPLATE | property sets: Pset_CurtainWallCommon, Constraints, Dimensions, Horizontal Grid, Other, Phasing
          35 x IFCWINDOW | type IFCWINDOWSTYLE "21 x 17 M 2" | object type "21 x 17 M 2" | names: "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1033280", "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1033418", "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1033536" (+32 more) | material: "Glass" | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          35 x IFCWINDOW | type IFCWINDOWSTYLE "21 x 17 M 2" | object type "21 x 17 M 2" | names: "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1063129", "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1063166", "AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1066519" (+32 more) | material: "Glass" | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "6 x 6 M" | object type "6 x 6 M" | names: "AR1242_IKKUNA:6 x 6 M:1073142" | material: materials ("Glass", "Sash") | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "6 x 6 M" | object type "6 x 6 M" | names: "AR1242_IKKUNA:6 x 6 M:1073464" | material: materials ("Glass", "Sash") | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCROOF | object type "Basic Roof:AR1261_VK-RAKENNE Huopakatto, rakenne 125mm" | names: "Basic Roof:AR1261_VK-RAKENNE Huopakatto, rakenne 125mm:1073682", "Basic Roof:AR1261_VK-RAKENNE Huopakatto, rakenne 125mm:1082492", "Basic Roof:AR1261_VK-RAKENNE Huopakatto, rakenne 125mm:1137144" | parts: 22 IFCSLAB | property sets: Pset_RoofCommon, Constraints, Construction, Dimensions, Other, Phasing
          1 x IFCSLAB | object type "Floor:AR1236_YP Betoni 200mm, eriste 150m" | FLOOR | names: "Floor:AR1236_YP Betoni 200mm, eriste 150m:1136168" | material: layers "Floor:AR1236_YP Betoni 200mm, eriste 150m" ("Mineral Wool" 150., "Default Floor" 200.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Other, Phasing, Structural
          4 x IFCRAILING | object type "Railing:AR1314_KAIDE Metalli, pyöreä 900mm" | names: "Railing:AR1314_KAIDE Metalli, pyöreä 900mm:1008323", "Railing:AR1314_KAIDE Metalli, pyöreä 900mm:1008585", "Railing:AR1314_KAIDE Metalli, pyöreä 900mm:1020405" (+1 more) | property sets: Pset_RailingCommon, Constraints, Dimensions, Other, Phasing, Construction

Types
  IFCWALLTYPE "Basic Wall:AR1311_VS NKH 130mm" | STANDARD | 141 occurrences | material: layers "Basic Wall:AR1311_VS NKH 130mm" ("Brick, WHITE" 130.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 1 occurrence | material: "Brick, WHITE" | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 1 occurrence | material: "Brick, WHITE" | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 1 occurrence | material: "Brick, WHITE" | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 1 occurrence | material: "Brick, GRAY" | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCURTAINWALLTYPE "Curtain Wall:AR1312_VS-LASI" | 44 occurrences | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCDOORSTYLE "9 x 20 M" | 2 occurrences | material: materials ("Cherry", "Metal - Stainless Steel", "Metal - Painted - Grey", "Glass") | property sets: 1315_VÄLIOVI Iso lasiaukko:9 x 20 M:560063, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:AR1241_US 1 420mm" | STANDARD | 17 occurrences | material: layers "Basic Wall:AR1241_US 1 420mm" ("Brick, GRAY" 90., "Air" 40., "Plywood, Sheathing" 30., "Concrete - Cast-in-Place Concrete" 170., "Brick, WHITE" 90.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCWALLTYPE "Basic Wall:AR1212_PERUSMUURI" | STANDARD | 10 occurrences | material: layers "Basic Wall:AR1212_PERUSMUURI" ("Concrete, Cast In Situ" 150., "Mineral Wool" 76., "Concrete, Cast In Situ" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:AR1311_VS Betoni 160mm" | STANDARD | 7 occurrences | material: layers "Basic Wall:AR1311_VS Betoni 160mm" ("Concrete, Cast In Situ" 160.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "9 x 21 M" | SINGLE_SWING_RIGHT | 30 occurrences | material: materials ("Door - Frame White", "Door - Panel White") | property sets: 1315_VÄLIOVI Puu, umpi:9 x 21 M:920526, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "9 x 21 M" | SINGLE_SWING_LEFT | 29 occurrences | material: materials ("Door - Frame White", "Door - Panel White") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "9 x 21 M" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Panel White", "Door - Frame White") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "7 x 21 M" | SINGLE_SWING_LEFT | 3 occurrences | material: materials ("Door - Frame White", "Door - Panel White") | property sets: 1315_VÄLIOVI Puu, umpi:7 x 21 M:922781, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "9 x 21 M" | SINGLE_SWING_RIGHT | 2 occurrences | material: materials ("Door - Frame White", "Door - Panel White") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "8 x 21 M" | SINGLE_SWING_RIGHT | 5 occurrences | material: materials ("Door - Frame", "Door - Panel") | property sets: 1315_VÄLIOVI Puu, umpi:8 x 21 M:923394, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 3 occurrences | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 1 occurrence | material: "Brick, WHITE" | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 1 occurrence | material: "Brick, WHITE" | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 1 occurrence | material: "Brick, WHITE" | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 1 occurrence | material: "Brick, WHITE" | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 1 occurrence | material: "Brick, GRAY" | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 1 occurrence | material: "Brick, GRAY" | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 1 occurrence | material: "Brick, GRAY" | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCOLUMNTYPE "300mm" | element type "300mm" | COLUMN | 1 occurrence | material: "Brick, GRAY" | property sets: Dimensions, Graphics, Identity Data, Other
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCCOLUMNTYPE "380 x 380mm" | element type "380 x 380mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Dimensions, Identity Data, Other, Structural
  IFCWALLTYPE "Basic Wall:AR1311_VS Betoni 210mm" | STANDARD | 1 occurrence | material: layers "Basic Wall:AR1311_VS Betoni 210mm" ("Concrete, Cast In Situ" 210.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:AR1311_VS Betoni 300mm" | STANDARD | 1 occurrence | material: layers "Basic Wall:AR1311_VS Betoni 300mm" ("Concrete, Cast In Situ" 300.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:AR1311_VS Betoni 420mm" | STANDARD | 6 occurrences | material: layers "Basic Wall:AR1311_VS Betoni 420mm" ("Concrete, Cast In Situ" 420.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:AR1311_VS Betoni 200mm" | STANDARD | 1 occurrence | material: layers "Basic Wall:AR1311_VS Betoni 200mm" ("Concrete, Cast In Situ" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "9 x 21 M" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Door - Frame White", "Door - Panel White") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:AR1311_VS Metalli, levyverhous 105mm" | STANDARD | 8 occurrences | material: layers "Basic Wall:AR1311_VS Metalli, levyverhous 105mm" ("Stainless Steel" 2.5, "Steel, 45-345" 100., "Stainless Steel" 2.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "8 x 21 M" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "8 x 21 M" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "9 x 21 M" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Frame White", "Door - Panel White") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "10 x 22 M" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Door - Frame White", "Door - Panel White") | property sets: 1315_VÄLIOVI Puu, umpi:10 x 22 M:935023, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "15 x 22 M" | DOUBLE_DOOR_SINGLE_SWING | 2 occurrences | material: materials ("Puu - tammi, höylätty", "NCS S 1502-G50Y Helmenharmaa, matta, ruisku") | property sets: 1315_VÄLIOVI Umpipariovi:15 x 22 M:939756, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCCURTAINWALLTYPE "Curtain Wall:AR1313_VS-ERITYIS Kevyt väliseinä, metalli runko" | 2 occurrences | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCDOORSTYLE "18 x 21 M" | 1 occurrence | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCCURTAINWALLTYPE "Curtain Wall:AR1245_LASIUS" | 5 occurrences | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCDOORSTYLE "19 x 21 M" | 1 occurrence | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "16 x 22 M" | 3 occurrences | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "18 x 21 M" | 1 occurrence | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "19 x 21 M" | 1 occurrence | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "21 x 17 M 2" | 63 occurrences | material: "Glass" | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1030634
  IFCWINDOWSTYLE "21 x 15 M 2" | 3 occurrences | material: "Glass" | property sets: AR1242_IKKUNA 2 x lasiaukko, 6:21 x 15 M 2:1050272, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCWINDOWSTYLE "21 x 17 M 2" | 64 occurrences | material: "Glass" | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1063054
  IFCWINDOWSTYLE "6 x 6 M" | 2 occurrences | material: materials ("Glass", "Sash") | property sets: AR1242_IKKUNA:6 x 6 M:1073142, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "6 x 6 M" | 2 occurrences | material: materials ("Glass", "Sash") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "10 x 23 M" | 1 occurrence | material: materials ("Cherry", "Metal - Stainless Steel", "Finish - White", "Glass") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "5 x 15 M 2" | 1 occurrence | material: materials ("Glass", "Sash") | property sets: AR1242_IKKUNA:5 x 15 M 2:1086714, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:AR1311_VS Puu 140mm" | STANDARD | 2 occurrences | material: layers "Basic Wall:AR1311_VS Puu 140mm" ("Gypsum Wall Board" 21., "Softwood, Lumber" 98., "Gypsum Wall Board" 21.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "6 x 21 M" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: 1315_VÄLIOVI Puu, umpi:6 x 21 M:952607, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "19 x 21 M" | 1 occurrence | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "16 x 22 M" | 1 occurrence | material: materials ("Metal - Stainless Steel", "Cherry", "Metal - Painted - Grey", "Glass") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "8 x 22 M" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Door - Frame White", "Door - Panel White") | property sets: 1315_VÄLIOVI Puu, umpi:8 x 22 M:980131, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes

Property sets
  Other | properties | on 438 objects (438 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
    Family Name = "Rectangular Mullion" (IFCTEXT)
  Other | properties | on 359 objects (359 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
    Family = "Rectangular Mullion: 50 x 150mm" (IFCLABEL)
    Family and Type = "Rectangular Mullion: 50 x 150mm" (IFCLABEL)
    Host Id = "Curtain Wall: AR1312_VS-LASI" (IFCLABEL)
    Type = "Rectangular Mullion: 50 x 150mm" (IFCLABEL)
    Type Id = "Rectangular Mullion: 50 x 150mm" (IFCLABEL)
  Other | properties | on 141 objects (139 IFCWALLSTANDARDCASE, 2 IFCWALL)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: AR1311_VS NKH 130mm" (IFCLABEL)
    Family and Type = "Basic Wall: AR1311_VS NKH 130mm" (IFCLABEL)
    Type = "Basic Wall: AR1311_VS NKH 130mm" (IFCLABEL)
    Type Id = "Basic Wall: AR1311_VS NKH 130mm" (IFCLABEL)
  Other | properties | on 104 objects (104 IFCPLATE)
    Category = "Curtain Panels" (IFCLABEL)
    Family = "System Panel: Glazed" (IFCLABEL)
    Family and Type = "System Panel: Glazed" (IFCLABEL)
    Host Id = "Curtain Wall: AR1312_VS-LASI" (IFCLABEL)
    Type = "System Panel: Glazed" (IFCLABEL)
    Type Id = "System Panel: Glazed" (IFCLABEL)
  Other | properties | on 66 objects (64 IFCWINDOW, 2 IFCOPENINGELEMENT)
    Category = "Windows" (IFCLABEL)
    Family = "AR1242_IKKUNA 2 x lasiaukko, 6: 21 x 17 M 2" (IFCLABEL)
    Family and Type = "AR1242_IKKUNA 2 x lasiaukko, 6: 21 x 17 M 2" (IFCLABEL)
    Head Height = 2625. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: AR1241_US 1 420mm" (IFCLABEL)
    Type = "AR1242_IKKUNA 2 x lasiaukko, 6: 21 x 17 M 2" (IFCLABEL)
    Type Id = "AR1242_IKKUNA 2 x lasiaukko, 6: 21 x 17 M 2" (IFCLABEL)
  Other | properties | on 61 objects (57 IFCWINDOW, 4 IFCOPENINGELEMENT)
    Category = "Windows" (IFCLABEL)
    Family = "AR1242_IKKUNA 2 x lasiaukko, 6: 21 x 17 M 2" (IFCLABEL)
    Family and Type = "AR1242_IKKUNA 2 x lasiaukko, 6: 21 x 17 M 2" (IFCLABEL)
    Head Height = 2725. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: AR1241_US 1 420mm" (IFCLABEL)
    Type = "AR1242_IKKUNA 2 x lasiaukko, 6: 21 x 17 M 2" (IFCLABEL)
    Type Id = "AR1242_IKKUNA 2 x lasiaukko, 6: 21 x 17 M 2" (IFCLABEL)
  Other | properties | on 60 objects (60 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "1315_VÄLIOVI Puu, umpi: 9 x 21 M" (IFCLABEL)
    Family and Type = "1315_VÄLIOVI Puu, umpi: 9 x 21 M" (IFCLABEL)
    Head Height = 2032. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: AR1311_VS NKH 130mm" (IFCLABEL)
    Type = "1315_VÄLIOVI Puu, umpi: 9 x 21 M" (IFCLABEL)
    Type Id = "1315_VÄLIOVI Puu, umpi: 9 x 21 M" (IFCLABEL)
  Other | properties | on 52 objects (52 IFCCOLUMN)
    Category = "Structural Columns" (IFCLABEL)
    Family = "AR1233_PILARI Betoni, neliö: 380 x 380mm" (IFCLABEL)
    Family and Type = "AR1233_PILARI Betoni, neliö: 380 x 380mm" (IFCLABEL)
    Type = "AR1233_PILARI Betoni, neliö: 380 x 380mm" (IFCLABEL)
    Type Id = "AR1233_PILARI Betoni, neliö: 380 x 380mm" (IFCLABEL)
  Other: 75 more contents on 412 objects not shown
  Constraints | properties | on 438 objects (438 IFCMEMBER)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 388 objects (298 IFCMEMBER, 90 IFCPLATE)
    Level = "Level: 1.krs Lattia" (IFCLABEL)
  Constraints | properties | on 180 objects (140 IFCMEMBER, 40 IFCPLATE)
    Level = "Level: 2.krs Lattia" (IFCLABEL)
  Constraints | properties | on 66 objects (64 IFCWINDOW, 2 IFCOPENINGELEMENT)
    Level = "Level: 2.krs Lattia" (IFCLABEL)
    Sill Height = 1125. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 61 objects (57 IFCWINDOW, 4 IFCOPENINGELEMENT)
    Level = "Level: 1.krs Lattia" (IFCLABEL)
    Sill Height = 1225. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 57 objects (54 IFCDOOR, 3 IFCOPENINGELEMENT)
    Level = "Level: 1.krs Lattia" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 42 objects (41 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Base Constraint = "Level: 1.krs Lattia" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 2.krs Lattia" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = TRUE (IFCBOOLEAN)
    Unconnected Height = 3400. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 40 objects (39 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Base Constraint = "Level: 1.krs Lattia" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Exterior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 2.krs Lattia" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = TRUE (IFCBOOLEAN)
    Unconnected Height = 3400. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints: 169 more contents on 374 objects not shown
  Dimensions | properties | on 403 objects (403 IFCMEMBER)
    Width on side 1 = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    Width on side 2 = 25. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 133 objects (127 IFCWINDOW, 6 IFCOPENINGELEMENT)
    Area = 3.75625000000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0855000000000002 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 76 objects (76 IFCMEMBER)
    Area = 0.2175 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 1050. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.007875 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 76 objects (76 IFCMEMBER)
    Area = 0.2175 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 1050. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.00787499999999999 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 66 objects (66 IFCPLATE)
    Area = 0.877499999999999 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 975. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0219375 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Width = 899.999999999999 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 66 objects (66 IFCMEMBER)
    Area = 0.1875 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 899.999999999998 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.00674999999999998 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 63 objects (63 IFCDOOR)
    Area = 3.04983899999998 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.114321079999999 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 47 objects (47 IFCCOLUMN)
    Area = 5.3124 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 6800. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.98192 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 422 more contents on 693 objects not shown
  Phasing | properties | on 1205 objects (438 IFCMEMBER, 192 IFCWALLSTANDARDCASE, 135 IFCWINDOW, 130 IFCPLATE)
    Phase Created = "Phase 1" (IFCLABEL)
  Structural | properties | on 210 objects (173 IFCWALLSTANDARDCASE, 35 IFCCURTAINWALL, 2 IFCWALL)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Structural | properties | on 52 objects (52 IFCCOLUMN)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Bottom Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Top Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
  Structural | properties | on 18 objects (18 IFCWALLSTANDARDCASE)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Exterior Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Interior Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Structural = TRUE (IFCBOOLEAN)
    Structural Usage = "Bearing" (IFCIDENTIFIER)
  Structural | properties | on 17 objects (17 IFCBEAM) | on 52 type objects
    Section Shape = 0 (IFCINTEGER)
  Structural | properties | on 16 objects (16 IFCCURTAINWALL)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Structural = TRUE (IFCBOOLEAN)
    Structural Usage = "Bearing" (IFCIDENTIFIER)
  Structural | properties | on 12 objects (12 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Structural | properties | on 2 objects (2 IFCSTAIR)
    Rebar Cover = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
  Structural | properties | on 2 objects (2 IFCBEAM)
    Cut Length = 12210.1212270386 (IFCLENGTHMEASURE) [MILLI METRE]
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    End Attachment Type = "End Elevation" (IFCIDENTIFIER)
    Rebar Cover - Bottom Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Top Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Start Attachment Type = "End Elevation" (IFCIDENTIFIER)
    Structural Usage = "Girder" (IFCIDENTIFIER)
  Structural: 16 more contents on 16 objects not shown
  Pset_WallCommon | properties | on 81 objects (79 IFCWALLSTANDARDCASE, 2 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "AR1311_VS NKH 130mm" (IFCIDENTIFIER)
    ThermalTransmittance = 4.15384615384615 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 52 objects (52 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "AR1311_VS NKH 130mm" (IFCIDENTIFIER)
    ThermalTransmittance = 4.15384615384615 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 15 objects (15 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "AR1241_US 1 420mm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.451191827468786 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 10 objects (10 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "AR1212_PERUSMUURI" (IFCIDENTIFIER)
    ThermalTransmittance = 3.48666666666667 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 8 objects (8 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "AR1311_VS NKH 130mm" (IFCIDENTIFIER)
    ThermalTransmittance = 4.15384615384615 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 6 objects (6 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "AR1311_VS Metalli, levyverhous 105mm" (IFCIDENTIFIER)
    ThermalTransmittance = 395.121951219512 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "AR1311_VS Betoni 160mm" (IFCIDENTIFIER)
    ThermalTransmittance = 6.5375 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "AR1311_VS Betoni 420mm" (IFCIDENTIFIER)
    ThermalTransmittance = 2.49047619047619 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon: 8 more contents on 14 objects not shown
  Pset_ColumnCommon | properties | on 51 objects (51 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "380 x 380mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 13 objects (13 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "300mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "300mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "380 x 380mm" (IFCIDENTIFIER)
  Identity Data | properties | on 403 objects (403 IFCMEMBER)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "50 x 150mm" (IFCTEXT)
  Identity Data | properties | on 81 objects (47 IFCCOLUMN, 16 IFCCURTAINWALL, 10 IFCWALLSTANDARDCASE, 8 IFCBEAM)
    Comments = "" (IFCTEXT)
  Identity Data | properties | on 20 objects (20 IFCMEMBER)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "200 x 150mm" (IFCTEXT)
  Identity Data | properties | on 17 objects (17 IFCBEAM)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "23.25.30.11.14.14" (IFCTEXT)
    OmniClass Title = "Beams" (IFCTEXT)
    Type Name = "380 x 520mm 2" (IFCTEXT)
  Identity Data | properties | on 15 objects (15 IFCMEMBER)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "70 x 150mm" (IFCTEXT)
  Identity Data | properties | on 10 objects (10 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "AR1235_VP Betoni 120mm" (IFCTEXT)
  Identity Data | properties | on 8 objects (8 IFCRAILING)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "AR1314_KAIDE Metalli, pyöreä 900mm" (IFCTEXT)
  Identity Data | properties | on 4 objects (4 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "AR1261_VK-RAKENNE Huopakatto, rakenne 125mm" (IFCTEXT)
  Identity Data: 264 more contents on 249 objects not shown
  Pset_CurtainWallCommon | properties | on 44 objects (44 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "AR1312_VS-LASI" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 5 objects (5 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "AR1245_LASIUS" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 2 objects (2 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "AR1313_VS-ERITYIS Kevyt väliseinä, metalli runko" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 114 objects (114 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Glazed" (IFCIDENTIFIER)
    ThermalTransmittance = 6.7069 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_PlateCommon | properties | on 16 objects (16 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Solid" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_MemberCommon | properties | on 152 objects (152 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 1050. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 66 objects (66 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 899.999999999998 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 33 objects (33 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 900.000000000002 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 21 objects (21 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 1000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 11 objects (11 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 1015. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 10 objects (10 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 2400. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 10 objects (10 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "200 x 150mm" (IFCIDENTIFIER)
    Span = 1840. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 10 objects (10 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "200 x 150mm" (IFCIDENTIFIER)
    Span = 619.999999999999 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon: 48 more contents on 125 objects not shown
  Horizontal Grid | properties | on 49 objects (49 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Horizontal Grid | properties | on 2 objects (2 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 1 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Horizontal Grid | properties | on 1 type object
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
  Horizontal Grid | properties | on 1 type object
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "Fixed Distance" (IFCIDENTIFIER)
    Spacing = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
  Horizontal Grid | properties | on 1 type object
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
    Spacing = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 50 objects (50 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 1 object (1 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 2 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 1 type object
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
  Vertical Grid | properties | on 1 type object
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "Maximum Spacing" (IFCIDENTIFIER)
    Spacing = 1524. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 1 type object
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
    Spacing = 3350. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_DoorCommon | properties | on 60 objects (60 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "9 x 21 M" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 7 objects (7 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "8 x 21 M" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 4 objects (4 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "9 x 21 M" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 4 objects (4 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "16 x 22 M" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 3 objects (3 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "7 x 21 M" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "9 x 20 M" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "15 x 22 M" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "19 x 21 M" (IFCIDENTIFIER)
  Pset_DoorCommon: 7 more contents on 7 objects not shown
  Construction | properties | on 403 objects (403 IFCMEMBER)
    Corner Mullion = FALSE (IFCBOOLEAN)
    Position = "Perpendicular to Face" (IFCLABEL)
    Thickness = 150. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 35 objects (35 IFCMEMBER)
    Corner Mullion = FALSE (IFCBOOLEAN)
    Position = "Perpendicular to Face" (IFCLABEL)
    Profile = "System Mullion Profile: Rectangular" (IFCLABEL)
    Thickness = 150. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 17 objects (12 IFCDOOR, 5 IFCOPENINGELEMENT)
    Dry Wall Frame = FALSE (IFCBOOLEAN)
    Masonry Frame = TRUE (IFCBOOLEAN)
    Masonry Inset = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    Swing Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Threshold = TRUE (IFCBOOLEAN)
  Construction | properties | on 10 objects (10 IFCSLAB)
    Default Thickness = 120. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Construction | properties | on 8 objects (8 IFCRAILING)
    Angled Joins = "Add Vertical/Horizontal Segments" (IFCIDENTIFIER)
    Baluster Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Landing Height Adjustment = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail Connections = "Trim" (IFCIDENTIFIER)
    Railing Height = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Tangent Joins = "Extend Rails to Meet" (IFCIDENTIFIER)
    Use Landing Height Adjustment = "No" (IFCIDENTIFIER)
  Construction | properties | on 4 objects (4 IFCROOF)
    Default Thickness = 125. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    Begin with Riser = TRUE (IFCBOOLEAN)
    End with Riser = FALSE (IFCBOOLEAN)
    Extend Below Riser Base = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 2 objects (2 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 8275. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction: 21 more contents on 8 objects not shown
  Materials and Finishes | properties | on 403 objects (403 IFCMEMBER)
    Material = "NCS S 0502-Y Valkoinen, matta, ruisku" (IFCLABEL)
  Materials and Finishes | properties | on 52 objects (52 IFCCOLUMN) | on 1 type object
    Structural Material = "Concrete - Cast-in-Place Concrete" (IFCLABEL)
  Materials and Finishes | properties | on 35 objects (35 IFCMEMBER)
    Material = "Aluminium" (IFCLABEL)
  Materials and Finishes | properties | on 17 objects (17 IFCBEAM)
    Structural Material = "Concrete, Cast-in-Place gray" (IFCLABEL)
  Materials and Finishes | properties | on 3 objects (2 IFCDOOR, 1 IFCOPENINGELEMENT)
    Door Finish = "NCS S 1502-G50Y Helmenharmaa, matta, ruisku" (IFCLABEL)
    Frame Finish = "NCS S 1502-G50Y Helmenharmaa, matta, ruisku" (IFCLABEL)
  Materials and Finishes | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    Monolithic Material = "Concrete, Cast In Situ" (IFCLABEL)
  Materials and Finishes | properties | on 9 type objects
    Door Material = "Door - Panel White" (IFCLABEL)
    Frame Material = "Door - Frame White" (IFCLABEL)
  Materials and Finishes | properties | on 8 type objects
    Exterior Pull Material = "Metal - Stainless Steel" (IFCLABEL)
    Frame Material = "Metal - Painted - Grey" (IFCLABEL)
    Glass Stop Material = "Metal - Painted - Grey" (IFCLABEL)
    Panel Material = "Metal - Painted - Grey" (IFCLABEL)
    Panic Bar Material = "Metal - Stainless Steel" (IFCLABEL)
    Threshold Material = "Cherry" (IFCLABEL)
  Materials and Finishes: 8 more contents on 0 objects not shown
  Pset_SlabCommon | properties | on 9 objects (9 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "AR1235_VP Betoni 120mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 5 objects (5 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 4.21457593324017 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "AR1261_VK-RAKENNE Huopakatto, rakenne 125mm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.246913580246914 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 4.21457593324025 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "AR1261_VK-RAKENNE Huopakatto, rakenne 125mm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.246913580246914 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "AR1261_VK-RAKENNE Huopakatto, rakenne 125mm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.246913580246914 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "AR1236_YP Betoni 200mm, eriste 150m" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 2.3721398604739 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "AR1261_VK-RAKENNE Huopakatto, rakenne 125mm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.246913580246914 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 2.47611314115682 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "AR1261_VK-RAKENNE Huopakatto, rakenne 125mm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.246913580246914 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 8.96310316197633 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "AR1261_VK-RAKENNE Huopakatto, rakenne 125mm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.246913580246914 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon: 4 more contents on 7 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCDOOR)
    Manufacturer = "-" (IFCLABEL)
  Graphics | properties | on 16 objects (12 IFCSLAB, 4 IFCROOF) | on 21 type objects
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Graphics | properties | on 3 objects (2 IFCDOOR, 1 IFCOPENINGELEMENT)
    3D Käyntiovi_aukeamiskulma = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    3D Sivuovi_aukeamiskulma = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Threshold Type = "Kynnys_kyntteellinen" (IFCLABEL)
  Graphics | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    Center Mark Visible = TRUE (IFCBOOLEAN)
  Graphics | properties | on 2 objects (2 IFCSTAIR)
    Cut Mark Type = "Stair Cut Mark: Single Zigzag" (IFCLABEL)
  Graphics | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Graphics | properties | on 4 type objects
    Coarse Scale Fill Color = 0 (IFCINTEGER)
    Coarse Scale Fill Pattern = "Concrete" (IFCLABEL)
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "380 x 520mm 2" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 103337.024647504 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "380 x 520mm 2" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 8776.11794396379 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "380 x 520mm 2" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 4829.11266098603 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "380 x 520mm 2" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 107158.032781138 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "380 x 520mm 2" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 95959.7720602929 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "380 x 520mm 2" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 91003.6549461503 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "380 x 520mm 2" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 103830.242741393 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "380 x 520mm 2" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 76659.786827314 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon: 9 more contents on 9 objects not shown
  Geometric Position | properties | on 17 objects (17 IFCBEAM)
    Join Status = "Both joins enabled" (IFCIDENTIFIER)
    y Justification = "Origin" (IFCIDENTIFIER)
    y Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    yz Justification = "Uniform" (IFCIDENTIFIER)
    z Justification = "Top" (IFCIDENTIFIER)
    z Offset Value = 3400. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 19. (IFCCOUNTMEASURE)
    NumberOfTreads = 19. (IFCCOUNTMEASURE)
    Reference = "AR1237_PORRAS Betoni" (IFCIDENTIFIER)
    RiserHeight = 178.947368421053 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 280. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 19. (IFCCOUNTMEASURE)
    NumberOfTreads = 19. (IFCCOUNTMEASURE)
    Reference = "190mm Depth" (IFCIDENTIFIER)
    RiserHeight = 178.947368421053 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 280. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 280. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WaistThickness = 1000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 500. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_WindowCommon | properties | on 127 objects (127 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "21 x 17 M 2" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 4 objects (4 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "6 x 6 M" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "21 x 15 M 2" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "5 x 15 M 2" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 4.12119960403015 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "AR1261_VK-RAKENNE Huopakatto, rakenne 125mm" (IFCIDENTIFIER)
    TotalArea = 4.1219933591869 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 2.20499999999999 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "AR1261_VK-RAKENNE Huopakatto, rakenne 125mm" (IFCIDENTIFIER)
    TotalArea = 2.20499999999999 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 434.033329717111 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "AR1261_VK-RAKENNE Huopakatto, rakenne 125mm" (IFCIDENTIFIER)
    TotalArea = 434.779985148994 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 1329.99638172466 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "AR1261_VK-RAKENNE Huopakatto, rakenne 125mm" (IFCIDENTIFIER)
    TotalArea = 1332.89735296552 (IFCAREAMEASURE) [SQUARE_METRE]
  Slab Shape Edit | properties | on 2 objects (2 IFCROOF)
    Curved Edge Condition = 0 (IFCINTEGER)
  Pset_RailingCommon | properties | on 8 objects (8 IFCRAILING)
    Height = 900. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "AR1314_KAIDE Metalli, pyöreä 900mm" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 2 (IFCINTEGER)
  Analytical Properties | properties | on 12 objects (12 IFCSLAB)
    Absorptance = 0.1 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
  Analytical Properties | properties | on 4 objects (4 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.246913580246914 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 4.05 (IFCREAL)
    Thermal mass = 42620.42 (IFCREAL)
  Analytical Properties | properties | on 13 type objects
    Analytic Construction = "<None>" (IFCTEXT)
  Analytical Properties | properties | on 13 type objects
    Analytic Construction = "Metal" (IFCTEXT)
    Heat Transfer Coefficient (U) = 3.7021 (IFCREAL)
    Solar Heat Gain Coefficient = 0. (IFCREAL)
    Thermal Resistance (R) = 0.270116960643959 (IFCREAL)
    Visual Light Transmittance = 0. (IFCREAL)
  Analytical Properties | properties | on 3 type objects
    Analytic Construction = "1/8 in Pilkington single glazing" (IFCTEXT)
    Heat Transfer Coefficient (U) = 3.6886 (IFCREAL)
    Solar Heat Gain Coefficient = 0.78 (IFCREAL)
    Thermal Resistance (R) = 0.271105568508377 (IFCREAL)
    Visual Light Transmittance = 0.9 (IFCREAL)
  Analytical Properties | properties | on 2 type objects
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 3.48666666666667 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.286806883365201 (IFCREAL)
    Thermal mass = 453330. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 4.15384615384615 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.240740740740741 (IFCREAL)
    Thermal mass = 169260. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.451191827468786 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 2.21635220125786 (IFCREAL)
    Thermal mass = 257923.368 (IFCREAL)
  Analytical Properties: 6 more contents on 0 objects not shown
  Calculation Rules | properties | on 2 objects (2 IFCSTAIR)
    Maximum Riser Height = 180. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Run Width = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Tread Depth = 280. (IFCLENGTHMEASURE) [MILLI METRE]
  End Connection | properties | on 2 objects (2 IFCSTAIR)
    Connection Method = "Notch" (IFCIDENTIFIER)
    Horizontal Gap Distance = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    Notch Extension = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Notch Thickness = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Gap Distance = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  Supports | properties | on 2 objects (2 IFCSTAIR)
    Left Lateral Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Support = "None" (IFCIDENTIFIER)
    Middle Support = FALSE (IFCBOOLEAN)
    Middle Support Number = 0 (IFCINTEGER)
    Right Lateral Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Support = "None" (IFCIDENTIFIER)
  Risers | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    Riser = FALSE (IFCBOOLEAN)
    Riser Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Riser To Tread Connection = "Extend Riser Behind Tread" (IFCIDENTIFIER)
    Slanted = FALSE (IFCBOOLEAN)
  Treads | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    Apply Nosing Profile = "Front Only" (IFCIDENTIFIER)
    Nosing Length = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tread = FALSE (IFCBOOLEAN)
    Tread Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Handrail 1 | properties | on 8 objects (8 IFCRAILING)
    Position = "None" (IFCIDENTIFIER)
  Handrail 2 | properties | on 8 objects (8 IFCRAILING)
    Position = "None" (IFCIDENTIFIER)
  Top Rail | properties | on 8 objects (8 IFCRAILING)
    Height = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "Top Rail Type: Circular - 40mm" (IFCLABEL)
  Horizontal Mullions | properties | on 2 type objects
    Border 1 Type = "Rectangular Mullion: 50 x 150mm" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 50 x 150mm" (IFCLABEL)
    Interior Type = "Rectangular Mullion: 50 x 150mm" (IFCLABEL)
  Horizontal Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion: 70 x 150mm" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 70 x 150mm" (IFCLABEL)
    Interior Type = "Rectangular Mullion: 70 x 150mm" (IFCLABEL)
  Vertical Mullions | properties | on 2 type objects
    Border 1 Type = "Rectangular Mullion: 50 x 150mm" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 50 x 150mm" (IFCLABEL)
    Interior Type = "Rectangular Mullion: 50 x 150mm" (IFCLABEL)
  Vertical Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion: 200 x 150mm" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 200 x 150mm" (IFCLABEL)
    Interior Type = "Rectangular Mullion: 200 x 150mm" (IFCLABEL)
  1315_VÄLIOVI Iso lasiaukko:9 x 20 M:560063 | predefined | on 2 type objects
  1315_VÄLIOVI Puu, umpi:9 x 21 M:920526 | predefined | on 2 type objects
  1315_VÄLIOVI Puu, umpi:9 x 21 M:920580 | predefined | on 2 type objects
  1315_VÄLIOVI Puu, umpi:9 x 21 M:920780 | predefined | on 2 type objects
  1315_VÄLIOVI Puu, umpi:7 x 21 M:922781 | predefined | on 2 type objects
  1315_VÄLIOVI Puu, umpi:9 x 21 M:923096 | predefined | on 2 type objects
  1315_VÄLIOVI Puu, umpi:8 x 21 M:923394 | predefined | on 2 type objects
  1315_VÄLIOVI Puu, umpi:9 x 21 M:933242 | predefined | on 2 type objects
  1315_VÄLIOVI Puu, umpi:8 x 21 M:933462 | predefined | on 2 type objects
  1315_VÄLIOVI Puu, umpi:8 x 21 M:934362 | predefined | on 2 type objects
  1315_VÄLIOVI Puu, umpi:9 x 21 M:934944 | predefined | on 2 type objects
  1315_VÄLIOVI Puu, umpi:10 x 22 M:935023 | predefined | on 2 type objects
  1315_VÄLIOVI Umpipariovi:15 x 22 M:939756 | predefined | on 2 type objects
  1315_VÄLIOVI Pariovi kaksi lasiaukkoa:18 x 21 M:963938 | predefined | on 2 type objects
  1315_VÄLIOVI Pariovi kaksi lasiaukkoa:19 x 21 M:1009814 | predefined | on 2 type objects
  1315_VÄLIOVI Pariovi kaksi lasiaukkoa:16 x 22 M:972686 | predefined | on 2 type objects
  1315_VÄLIOVI Pariovi kaksi lasiaukkoa:18 x 21 M:1028795 | predefined | on 2 type objects
  1315_VÄLIOVI Pariovi kaksi lasiaukkoa:19 x 21 M:1029766 | predefined | on 2 type objects
  AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1030634 | predefined | on 1 type object
  AR1242_IKKUNA 2 x lasiaukko, 6:21 x 15 M 2:1050272 | predefined | on 1 type object
  AR1242_IKKUNA 2 x lasiaukko, 6:21 x 17 M 2:1063054 | predefined | on 1 type object
  AR1242_IKKUNA:6 x 6 M:1073142 | predefined | on 1 type object
  AR1242_IKKUNA:6 x 6 M:1073400 | predefined | on 1 type object
  1243_ULKOOVI Iso lasiaukolla:10 x 23 M:1082471 | predefined | on 2 type objects
  AR1242_IKKUNA:5 x 15 M 2:1086714 | predefined | on 1 type object
  1315_VÄLIOVI Puu, umpi:6 x 21 M:952607 | predefined | on 2 type objects
  1315_VÄLIOVI Pariovi kaksi lasiaukkoa:19 x 21 M:954973 | predefined | on 2 type objects
  1315_VÄLIOVI Pariovi kaksi lasiaukkoa:16 x 22 M:955166 | predefined | on 2 type objects
  1315_VÄLIOVI Puu, umpi:8 x 22 M:980131 | predefined | on 2 type objects